**Open Geospatial Consortium**

Submission Date: <yyyy-dd-mm>

Approval Date:   <yyyy-dd-mm>

Publication Date:   <yyyy-dd-mm>

External identifier of this OGC® document: <<http://www.opengis.net/def/doc-type/standard/1.0>>

Internal reference number of this OGC® document:    YY-nnnrx

Version: n.n.n

Category: OGC® <Implementation / Abstract Specification / Best Practice>

Editor:   Ted Habermann

OGC GeoTIFF Standard

**Copyright notice**

Copyright © 2015 Open Geospatial Consortium  
To obtain additional rights of use, visit <http://www.opengeospatial.org/legal/>.

**Warning**

This document is not an OGC Standard. This document is distributed for review and comment. This document is subject to change without notice and may not be referred to as an OGC Standard.

Document type:    OGC® Standard

Document subtype:    if applicable

Document stage:    Draft

Document language:  English

Recipients of this document are invited to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation.

License Agreement

Permission is hereby granted by the Open Geospatial Consortium, ("Licensor"), free of charge and subject to the terms set forth below, to any person obtaining a copy of this Intellectual Property and any associated documentation, to deal in the Intellectual Property without restriction (except as set forth below), including without limitation the rights to implement, use, copy, modify, merge, publish, distribute, and/or sublicense copies of the Intellectual Property, and to permit persons to whom the Intellectual Property is furnished to do so, provided that all copyright notices on the intellectual property are retained intact and that each person to whom the Intellectual Property is furnished agrees to the terms of this Agreement.

If you modify the Intellectual Property, all copies of the modified Intellectual Property must include, in addition to the above copyright notice, a notice that the Intellectual Property includes modifications that have not been approved or adopted by LICENSOR.

THIS LICENSE IS A COPYRIGHT LICENSE ONLY, AND DOES NOT CONVEY ANY RIGHTS UNDER ANY PATENTS THAT MAY BE IN FORCE ANYWHERE IN THE WORLD.

THE INTELLECTUAL PROPERTY IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, AND NONINFRINGEMENT OF THIRD PARTY RIGHTS. THE COPYRIGHT HOLDER OR HOLDERS INCLUDED IN THIS NOTICE DO NOT WARRANT THAT THE FUNCTIONS CONTAINED IN THE INTELLECTUAL PROPERTY WILL MEET YOUR REQUIREMENTS OR THAT THE OPERATION OF THE INTELLECTUAL PROPERTY WILL BE UNINTERRUPTED OR ERROR FREE. ANY USE OF THE INTELLECTUAL PROPERTY SHALL BE MADE ENTIRELY AT THE USER’S OWN RISK. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR ANY CONTRIBUTOR OF INTELLECTUAL PROPERTY RIGHTS TO THE INTELLECTUAL PROPERTY BE LIABLE FOR ANY CLAIM, OR ANY DIRECT, SPECIAL, INDIRECT OR CONSEQUENTIAL DAMAGES, OR ANY DAMAGES WHATSOEVER RESULTING FROM ANY ALLEGED INFRINGEMENT OR ANY LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION OF CONTRACT, NEGLIGENCE OR UNDER ANY OTHER LEGAL THEORY, ARISING OUT OF OR IN CONNECTION WITH THE IMPLEMENTATION, USE, COMMERCIALIZATION OR PERFORMANCE OF THIS INTELLECTUAL PROPERTY.

This license is effective until terminated. You may terminate it at any time by destroying the Intellectual Property together with all copies in any form. The license will also terminate if you fail to comply with any term or condition of this Agreement. Except as provided in the following sentence, no such termination of this license shall require the termination of any third party end-user sublicense to the Intellectual Property which is in force as of the date of notice of such termination. In addition, should the Intellectual Property, or the operation of the Intellectual Property, infringe, or in LICENSOR’s sole opinion be likely to infringe, any patent, copyright, trademark or other right of a third party, you agree that LICENSOR, in its sole discretion, may terminate this license without any compensation or liability to you, your licensees or any other party. You agree upon termination of any kind to destroy or cause to be destroyed the Intellectual Property together with all copies in any form, whether held by you or by any third party.

Except as contained in this notice, the name of LICENSOR or of any other holder of a copyright in all or part of the Intellectual Property shall not be used in advertising or otherwise to promote the sale, use or other dealings in this Intellectual Property without prior written authorization of LICENSOR or such copyright holder. LICENSOR is and shall at all times be the sole entity that may authorize you or any third party to use certification marks, trademarks or other special designations to indicate compliance with any LICENSOR standards or specifications. This Agreement is governed by the laws of the Commonwealth of Massachusetts. The application to this Agreement of the United Nations Convention on Contracts for the International Sale of Goods is hereby expressly excluded. In the event any provision of this Agreement shall be deemed unenforceable, void or invalid, such provision shall be modified so as to make it valid and enforceable, and as so modified the entire Agreement shall remain in full force and effect. No decision, action or inaction by LICENSOR shall be construed to be a waiver of any rights or remedies available to it.

Contents

[1. Scope 2](#_Toc337499850)

[2. Conformance 2](#_Toc337499851)

[3. References 2](#_Toc337499852)

[4. Terms and Definitions 2](#_Toc337499853)

[5. Conventions 2](#_Toc337499854)

[6. Clauses not Containing Normative Material 2](#_Toc337499855)

[6.1 Clauses not containing normative material sub-clause 1 2](#_Toc337499856)

[6.1.1 Clauses not containing normative material sub-clause 2 2](#_Toc337499857)

[7. Clause containing normative material 2](#_Toc337499858)

[7.1 Requirement Class A or Requirement A 2](#_Toc337499859)

[7.2 Requirement Class B or Requirement B 2](#_Toc337499860)

[8. Media Types for any data encoding(s) 2](#_Toc337499861)

[A.1 Conformance class: AAAA (repeat as necessary) 2](#_Toc337499862)

Abstract

This profile specifies the requirements and encoding rules for using the Tagged Image File Format (TIFF) for the exchange of georeferenced imagery. It formalizes the existing community standard for the Geographic Tagged Image File Format (GeoTIFF) file format.

Keywords

The following are keywords to be used by search engines and document catalogues.

ogcdoc, OGC document, <tags separated by commas>

Preface

<Insert Preface Text here. Give OGC specific commentary: describe the technical content, reason for document, history of the document and precursors, and plans for future work. >

The GeoTIFF format was initially developed during the early 1990’s (N. Ritter & Ruth, 1997) in order to leverage a mature platform independent file format (TIFF) by adding metadata required for describing and using geographic image data. TIFF met the requirements for an underlying format, as it was lossless and extensible. In September 1994, SPOT Image Corp proposed a GeoTIFF structure that was limited to Universal Transverse Mercator (N. Ritter & Ruth, 1997). The proposed GeoTIFF specification has augmented and formalized by Niles and Ruth as Revision 1.0, specification version 1.8.2 in November 1995 (N. Ritter & Ruth, 1995). This specification is currently the official GeoTIFF specification (GeoTIFF, n.d).

The GeoTIFF format is used throughout the geospatial and earth science communities to share geographic image data. That usage inevitably leads to identification of new requirements and needs for profiles, extensions, and improvements to the original GeoTIFF Specification. The OGC is well established as a forum for standardization in the GeoTIFF producer and user communities and, as such, it provides an inclusive standardization process for those communities. This document is the first step in the process of integration of the GeoTIFF into that standardization process. Once GeoTIFF is ensconced in the OGC, the standard can be evolved using a formal process.

Suggested additions, changes, and comments on this standard are welcome and

encouraged. Such suggestions may be submitted by email message or by submitting an

official OGC Change Request using the online CR application:

https://portal.opengeospatial.org/public\_ogc/change\_request.php

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. The Open Geospatial Consortium shall not be held responsible for identifying any or all such patent rights.

*Recipients of this document are requested to submit, with their comments, notification of any relevant patent claims or other intellectual property rights of which they may be aware that might be infringed by any implementation of the standard set forth in this document, and to provide supporting documentation.*

Submitting organizations

The following organizations submitted this Document to the Open Geospatial Consortium (OGC):

The HDF Group

Submitters

All questions regarding this submission should be directed to the editor or the submitters:

|  |  |
| --- | --- |
| Name | Affiliation |
| Ted Habermann | The HDF Group |
|  |  |
|  |  |

# Scope

This OGC**®** Standard defines a set of TIFF tags provided to describe all "Cartographic" information associated with TIFF imagery that originates from satellite imaging systems, scanned aerial photography, scanned maps, digital elevation models, or as a result of geographic analyses. Its aim is to allow means for tying a raster image to a known model space or map projection, and for describing those projections. This OGC**®** Standard defines the Geographic Tagged Image File Format (GeoTIFF) file format and the requirements to which every GeoTIFF file must adhere. It focuses on updating the current GeoTIFF community specification and aligning it with current OGC standardization practice.

The tags documented in this spec are to be considered completely orthogonal to the raster-data descriptions of the TIFF spec, and impose no restrictions on how the standard TIFF tags are to be interpreted, which color spaces or compression types are to be used, etc.

# Conformance

This standard defines XXXX.

Requirements for N standardization target types are considered:

* AAAA
* BBBB

Conformance with this standard shall be checked using all the relevant tests specified in Annex A (normative) of this document. The framework, concepts, and methodology for testing, and the criteria to be achieved to claim conformance are specified in the OGC Compliance Testing Policies and Procedures and the OGC Compliance Testing web site[[1]](#footnote-1).

In order to conform to this OGC™interface standard, a software implementation shall choose to implement:

1. Any one of the conformance levels specified in Annex B (normative).
2. Any one of the Distributed Computing Platform profiles specified in Annexes TBD through TBD (normative).

All requirements-classes and conformance-classes described in this document are owned by the standard(s) identified.

# References

The following normative documents contain provisions that, through reference in this text, constitute provisions of this document. For dated references, subsequent amendments to, or revisions of, any of these publications do not apply. For undated references, the latest edition of the normative document referred to applies.

There are no normative references.

# Terms and Definitions

This document uses the terms defined in Sub-clause 5.3 of [OGC 06-121r8], which is based on the ISO/IEC Directives, Part 2, Rules for the structure and drafting of International Standards. In particular, the word “shall” (not “must”) is the verb form used to indicate a requirement to be strictly followed to conform to this standard.

For the purposes of this document, the following additional terms and definitions apply.

1. absolute accuracy

Closeness of coordinate value to the true or accepted valuein a specified reference system (in this profile, the reference system is the World Geodetic System 1984 (WGS84))

1. ASCII

[American Standard Code for Information Interchange] The predominant character set encoding of present-day computers.

1. band

A well-defined range of wavelengths, frequencies or energies of optical, electric or acoustic radiation. At the pixel level, a band is represented as one of the vector values of the pixel. At image level, band i of an image is the rectangular array of ith sample values from the pixel vectors.

1. cell

A rectangular area in Raster space, in which a single pixel value is filled.

1. code

representation of a label according to a specified scheme

1. coordinate

One of a sequence of numbers designating the position of a point in N-dimensional space

1. coordinate reference system

Coordinate system that is related to an object (of the real world) by a datum.

1. coordinate system

A set of mathematical rules for specifying how coordinates are to be assigned to points

1. coverage

Feature that acts as a function to return values from its range for any direct position within its spatial, temporal, or spatiotemporal domain. Examples include a digital image, raster map, and digital elevation matrix.

1. coverage geometry

Configuration of the domain of a coverage described in terms of coordinates.

1. data compression

Reducing the amount of storage space required to store a given amount of data, or reducing the length of message required to transfer a given amount of reduction in the number of bits used to represent source image data [ISO 10918-1] (JPEG Part 1) information. (data / image) compression

1. dataset

Identifiable collection of data.

1. datum

A parameter or set of parameters that define the position of the origin, the scale, and the orientation of a coordinate system

1. device space

A coordinate space referencing scanner, printers and display devices.

1. direct position

Position described by a single set of coordinates within a coordinate reference system.

1. domain

Well-defined set. Note, Domains are used to define the domain set and range set of operators and functions.

1. double

8-byte IEEE double precision floating point.

1. ellipsoid

A surface formed by the rotation of an ellipse about a main axis

1. EPSG

European Petroleum Survey Group.

1. evaluation

Determination of the values of a coverage at a direct position within the domain of the coverage.

1. flattening

A ratio of the difference between the semi-major (a) and semi-minor axis (b) of an ellipsoid to the semi-major axis; f = (a - b)/a

1. geocoding

A translation of one form of location into another

1. geographic coordinate system

A Geographic CS consists of a well-defined ellipsoidal datum, a Prime Meridian, and an angular unit, allowing the assignment of a Latitude-Longitude (and optionally, geodetic height) vector to a location on earth.

1. geokey

In GeoTIFF, a GeoKey is equivalent in function to a TIFF tag, but uses a different storage mechanism.

1. georectified grid

Rectified Grid: grid for which there is an affine transformation between the grid coordinates and the coordinates of an external coordinate reference system

1. georeferencing

geopositioning an object using a Correspondence Model derived from a set of points for which both ground and image coordinates are known

1. geotiff

A standard for storing georeference and geocoding information in a TIFF 6.0 compliant raster file.

1. grid

A network composed of two or more sets of curves in which the members of each set intersect the members of the other sets in an algorithmic way

1. grid

gridded data Network composed of two or more sets of curves in which the members of each set intersect the members of the other sets in a algorithmic way.

1. IEEE

Institute of Electrical and Electronics Engineers, Inc.

1. IFD

In TIFF format, an Image File Directory, containing all the TIFF tags for one image in the file (there may be more than one).

1. imagery

Representation of phenomena as images produced electronically and/or optical techniques.

1. meridian

An intersection of an ellipsoid by a plane containing the shortest axis of the ellipsoid

1. metadata

Data about data.

1. model space

A flat geometrical space used to model a portion of the earth.

1. mosaic

For purposes of this profile, a mosaic image is an image composed of two or more separately collected (sensed) images. Additional XML metadata may be used to identify the cut-lines (boundaries and parameters for the images used to compose the mosaic.

1. null value

Value having no value or existence.

1. orthorectified grid

Georectified grid created using ground control points and elevation data where constant scale is maintained throughout the grid.

1. parallel

Lines of constant latitude, parallel to the equator.

1. pixel

The smallest element of a digital image to which attributes are assigned

1. pixel

Smallest element of a digital image to which attributes are assigned.

NOTE 1 This term originated as a contraction of “picture element”.

NOTE 2 Related to the concept of a grid cell The intensity of each pixel is variable; in color systems, each pixel has typically three or four dimensions of variability such as red, green and blue, or cyan, magenta, yellow and black.

1. POSC

Petrotechnical Open Software Corporation.

1. prime meridian

A meridian from which the longitudes of other meridians are quantified

1. projected coordinate system

A coordinate reference system derived from a two-dimensional geodetic coordinate reference system by applying a map projection

1. projection

projected coordinate reference system: coordinate reference system derived from a two-dimensional geodetic coordinate reference system by applying a map projection

1. qualification layer

A qualification layer is a coverage consisting of graphics information associated to geospatial data together with associated metadata (these metadata mostly identify the meaning of colour codes used in graphics).

1. range

Set of feature attribute values associated by a function with the elements of the domain of a coverage.

1. raster space

Raster: usually rectangular pattern of parallel scanning lines forming or corresponding to the display on a cathode ray tube

1. rational

In TIFF format, a RATIONAL value is a fractional value represented by the ratio of two unsigned 4-byte integers.

1. rectified grid

Grid for which there is an affine transformation between the grid coordinates and the coordinates of an external coordinate reference system.

1. referenceable grid

Grid associated with a transformation that can be used to convert grid coordinate values to values of coordinates referenced to an external coordinate reference system

1. relative accuracy / relative positional accuracy

Evaluation of the random errors in determining the position of one point or feature with respect to another / closeness of coordinate difference value to the true or accepted value in a specified reference system

1. SDTS

The USGS Spatial Data Transmission Standard.

1. tag

In TIFF format, a tag is packet of numerical or ASCII values, which have a numerical "Tag" ID indicating their information content.

1. tessellation / tiling

Partitioning of a space into a set of conterminous subspaces having the same dimension as the space being partitioned

1. TIFF

Acronym for Tagged Image File Format; a platform-independent, extensive specification for storing raster data and ancillary information in a single file.

1. transparency mask

A Transparency Mask defines visible pixels of another image in the same TIFF file (that may be organised as an irregularly shaped region of visible pixels). The 1-bits define the visible pixels; the 0-bits define transparent pixels. (fdefinition based on TIFF specification)

1. USGS

US Geological Survey

# Conventions

None

# Clauses not Containing Normative Material

Paragraph

## Clauses not containing normative material sub-clause 1

Paragraph

### Clauses not containing normative material sub-clause 2

# Clause containing normative material

## Requirements Class GeoAsciiParamsTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeoAsciiParamsTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoAsciiParamsTag.count  *The GeoAsciiParamsTag MAY hold any number of key parameters with type = ASCII. (May not be necessary, the same as keyentry.count)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoAsciiParamsTag.ID  *The GeoAsciiParamsTag SHALL have ID = 34737* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoAsciiParamsTag.NULLRead  *Pipe characters (“|”) in the GeoAsciiParamsTag SHALL be converted NULL characters before returning strings to the client* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoAsciiParamsTag.NULLWrite  *NULL characters used to terminate strings in the GeoAsciiParamsTag SHALL be converted to a “|” (pipe) prior to being written into the GeoAsciiParamsTag* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoAsciiParamsTag.type  *The GeoAsciiParamsTag SHALL have type = ASCII* |

## Requirements Class GeodeticDatumGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.ArchaicDatum  *GeodeticDatumGeoKey values in the range 6900-6999 SHALL be Archaic Datum* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.EPSGDatum  *GeodeticDatumGeoKey values in the range 6200-6999 SHALL be EPSG Datum Based on EPSG Datum* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.EPSGEllipsoid  *GeodeticDatumGeoKey values in the range 6000-6199 SHALL be EPSG Datum Based on Ellipsoid only* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.obsolete  *GeodeticDatumGeoKey values in the range 1-1000 SHALL be obsolete EPSG/POSC Datum Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.private  *GeodeticDatumGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.reserved  *GeodeticDatumGeoKey values in the range 1001-5999 and 7000-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeodeticDatumGeoKey.WGSDatum  *GeodeticDatumGeoKey values in the range 6322-6327 SHALL be WGS Datum* |

## Requirements Class GeoDoubleParamsTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeoDoubleParamsTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoDoubleParamsTag.count  *The GeoDoubleParamsTag MAY hold any number of key parameters with type = double. (May not be necessary, the same as keyentry.count)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoDoubleParamsTag.ID  *The GeoDoubleParamsTag SHALL have ID = 34736* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoDoubleParamsTag.type  *The GeoDoubleParamsTag SHALL have type = DOUBLE (IEEE Double Precision)* |

## Requirements Class GeogAngularUnitsGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitsGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitsGeoKey.ID  *The GeogAngularUnitsGeoKey SHALL have ID = 2054* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitsGeoKey.type  *The GeogAngularUnitsGeoKey SHALL have type = SHORT* |

## Requirements Class GeogAngularUnitSizeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitSizeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitSizeGeoKey.ID  *The GeogAngularUnitSizeGeoKey SHALL have ID = 2055* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitSizeGeoKey.type  *The GeogAngularUnitSizeGeoKey SHALL have type = DOUBLE* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAngularUnitSizeGeoKey.units  *The units of the GeogAngularUnitSizeGeoKey SHALL be radians* |

## Requirements Class GeogAzimuthUnitsGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogAzimuthUnitsGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAzimuthUnitsGeoKey.ID  *The GeogAzimuthUnitsGeoKey SHALL have ID = 2060* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogAzimuthUnitsGeoKey.type  *The GeogAzimuthUnitsGeoKey SHALL have type = SHORT* |

## Requirements Class GeogCitationGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogCitationGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogCitationGeoKey.ID  *The GeogCitationGeoKey SHALL have ID = 2049* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogCitationGeoKey.type  *The GeogCitationGeoKey SHALL have type = ASCII* |

## Requirements Class GeogEllipsoidGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey.EPSGEllipsoid  *GeogEllipsoidGeoKey values in the range 7000-7999 SHALL be EPSG Ellipsoid Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey.ID  *The GeogEllipsoidGeoKey SHALL have ID = 2056* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey.obsolete  *GeogEllipsoidGeoKey values in the range 1-1000 SHALL be obsolete EPSG/POSC Datum Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey.private  *GeogEllipsoidGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey.reserved  *GeogEllipsoidGeoKey values in the range 1001-6999 and 8000-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogEllipsoidGeoKey.type  *The GeogEllipsoidGeoKey SHALL have type = SHORT* |

## Requirements Class GeogGeodeticDatumGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogGeodeticDatumGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogGeodeticDatumGeoKey.ID  *The GeogCitationGeoKey SHALL have ID = 2050* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogGeodeticDatumGeoKey.type  *The GeogCitationGeoKey SHALL have type = SHORT* |

## Requirements Class GeogInvFlatteningGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogInvFlatteningGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogInvFlatteningGeoKey.ID  *The GeogInvFlatteningGeoKey SHALL have ID = 2059* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogInvFlatteningGeoKey.type  *The GeogInvFlatteningGeoKey SHALL have type = DOUBLE* |

## Requirements Class GeogLinearUnitsGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.angular  *GeogLinearUnitsGeoKey values in the range 9100-9199 SHALL be EPSG angular units* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.ID  *The GeogLinearUnitsGeoKey SHALL have ID = 2052* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.linear  *GeogLinearUnitsGeoKey values in the range 9000-9099 SHALL be EPSG linear units* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.obsolete  *GeogLinearUnitsGeoKey values in the range 1-2000 SHALL be obsolete GeoTIFF Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.private  *GeogLinearUnitsGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.reserved  *GeogLinearUnitsGeoKey values in the range 2001-8999 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitsGeoKey.type  *The GeogLinearUnitsGeoKey SHALL have type = DOUBLE* |

## Requirements Class GeogLinearUnitSizeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitSizeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitSizeGeoKey.ID  *The GeogLinearUnitSizeGeoKey SHALL have ID = 2053* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitSizeGeoKey.type  *The GeogLinearUnitSizeGeoKey SHALL have type = DOUBLE* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogLinearUnitSizeGeoKey.units  *The units of the GeogLinearUnitSizeGeoKey SHALL be meters* |

## Requirements Class GeogPrimeMeridianGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey.EPSGEllipsoid  *GeogPrimeMeridianGeoKey values in the range 8000-8999 SHALL be EPSG Prime Meridian Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey.ID  *The GeogPrimeMeridianGeoKey SHALL have ID = 2051* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey.obsolete  *GeogPrimeMeridianGeoKey values in the range 1-100 SHALL be obsolete EPSG/POSC Datum Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey.private  *GeogPrimeMeridianGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey.reserved  *GeogPrimeMeridianGeoKey values in the range 101-7999 and 9000-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianGeoKey.type  *The GeogPrimeMeridianGeoKey SHALL have type = SHORT* |

## Requirements Class GeogPrimeMeridianLongGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianLongGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianLongGeoKey.ID  *The GeogPrimeMeridianLongGeoKey SHALL have ID = 2061* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianLongGeoKey.type  *The GeogPrimeMeridianLongGeoKey SHALL have type = DOUBLE* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogPrimeMeridianLongGeoKey.units  *The GeogPrimeMeridianLongGeoKey SHALL have units = GeogAngularUnits* |

## Requirements Class GeographicTypeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.DGIWGReference  *WGS84 + may include Reference document citation (EPSG, DGIWG Registry or [DMA TR 8350.2])* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.DGIWGValues  *SHALL be 4326 (GCS\_WGS84) or 4030 (GCSE\_WGS84, not recommended by GeoTIFF)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.EPSGDatum  *GeographicTypeGeoKey values in the range 4200-4999 SHALL be EPSG GCS Based on EPSG Datum* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.EPSGEllipsoid  *GeographicTypeGeoKey values in the range 4000-4199 SHALL be EPSG GCS Based on Ellipsoid only* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.ID  *The GeographicTypeGeoKey SHALL have ID = 2048* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.obsolete  *GeographicTypeGeoKey values in the range 1-1000 SHALL be obsolete EPSG/POSC Geographic Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.private  *GeographicTypeGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.reserved  *GeographicTypeGeoKey values in the range 1001-3999 and 5000-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeographicTypeGeoKey.type  *The GeographicTypeGeoKey SHALL have type = SHORT* |

## Requirements Class GeogSemiMajorAxisGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMajorAxisGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMajorAxisGeoKey.ID  *The GeogSemiMajorAxisGeoKey SHALL have ID = 2057* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMajorAxisGeoKey.type  *The GeogSemiMajorAxisGeoKey SHALL have type = DOUBLE* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMajorAxisGeoKey.units  *The units of the GeogSemiMajorAxisGeoKey SHALL be Geocentric CS linear Units* |

## Requirements Class GeogSemiMinorAxisGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMinorAxisGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMinorAxisGeoKey.ID  *The GeogSemiMinorAxisGeoKey SHALL have ID = 2058* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMinorAxisGeoKey.type  *The GeogSemiMinorAxisGeoKey SHALL have type = DOUBLE* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeogSemiMinorAxisGeoKey.units  *The units of the GeogSemiMinorAxisGeoKey HALL be Geocentric CS linear Units* |

## Requirements Class GeoKeyCode

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyCode | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyCode.undefined  *GeoKeys with a value of zero SHALL indicate intentionally omitted parameters* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyCode.userDefined  *GeoKeys with a value of 32767 SHALL indicate user-defined parameters* |

## Requirements Class GeoKeyDirectoryTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.count  *The GeoKeyDirectoryTag SHALL include at least 4 keys (short integers) as header information* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.ID  *The GeoKeyDirectoryTag SHALL have ID = 34735* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.keyDirectoryVersion  *The first unsigned short integer in the GeoKeyDirectoryTag SHALL hold the KeyDirectoryVersion.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.keyEntrySetCount  *The GeoKeyDirectoryTag SHALL hold NumberOfKeys KeyEntry Sets in addition to the header information* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.keyRevision  *The second unsigned short integer in the GeoKeyDirectoryTag SHALL hold the KeyRevision.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.minorRevision  *The third unsigned short integer in the GeoKeyDirectoryTag SHALL hold the MinorRevision.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.numberOfKeys  *The fourth unsigned short integer in the GeoKeyDirectoryTag SHALL hold the NumberOfKeys defined in the rest of the GeoKeyDirectoryTag.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyDirectoryTag.type  *The GeoKeyDirectoryTag SHALL have type = SHORT (2-byte unsigned integer)* |

## Requirements Class GeoKeyRange

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange.configuration  *GeoKey ID's in the range 1024-2047 SHALL be GeoTIFF Configuration Keys* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange.geographic  *GeoKey ID's in the range 2048-3071 SHALL be Geographic/Geocentric Coordinate System Parameter Keys* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange.projected  *GeoKey ID's in the range 3072-4095 SHALL be Projected Coordinate System Parameter Keys* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange.reserved  *GeoKey ID's in the range 0-1023 and 5120-32767 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange.reserved  *GeoKey ID's in the range 4096-5119 SHALL be Vertical Coordinate System Parameter Keys* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GeoKeyRange.reserved  *GeoKey ID's in the range 32768-65535 SHALL be for private use* |

## Requirements Class GTCitationGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GTCitationGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTCitationGeoKey.ID  *The GTCitationGeoKey SHALL have ID = 1026* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTCitationGeoKey.type  *The GTCitationGeoKey SHALL have type = ASCII* |

## Requirements Class GTModelTypeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.geocentric  *A value of 3 for the GTModelTypeGeoKey SHALL indicate a geocentric(X,Y,Z) coordinate system* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.geographic  *A value of 2 for the GTModelTypeGeoKey SHALL indicate a geographic latitude-longitude coordinate system* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.ID  *The GTModelTypeGeoKey SHALL have ID = 1024* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.private  *GTModelTypeGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.projected  *A value of 1 for the GTModelTypeGeoKey SHALL indicate a projected coordinate system* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.reserved  *GTModelTypeGeoKey values in the range 1-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTModelTypeGeoKey.type  *The GTModelTypeGeoKey SHALL have type = SHORT* |

## Requirements Class GTRasterTypeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey.ID  *The GTModelTypeGeoKey SHALL have ID = 1025* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey.private  *GTRasterTypeGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey.rasterPixelIsArea  *A value of 1 for the GTRasterTypeGeoKey SHALL indicate that this raster pixel is an area (for DGIWG profile, this is used by imagery products).* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey.rasterPixelIsPoint  *A value of 2 for the GTRasterTypeGeoKey SHALL indicate that this raster pixel is a point (for DGIWG profile, this is used for discrete coverage data including elevation data ).* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey.reserved  *GTRasterTypeGeoKey values in the range 1-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/GTRasterTypeGeoKey.type  *The GTModelTypeGeoKey SHALL have type = SHORT* |

## Requirements Class IntergraphMatrixTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/IntergraphMatrixTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/IntergraphMatrixTag.count  *The IntergraphMatrixTag SHALL hold sixteen or seventeen values* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/IntergraphMatrixTag.deprecated  *The IntergraphMatrixTag SHALL not be used* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/IntergraphMatrixTag.ID  *The IntergraphMatrixTag SHALL have ID = 33920* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/IntergraphMatrixTag.type  *The IntergraphMatrixTag SHALL have type = DOUBLE* |

## Requirements Class KeyEntrySet

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet.count  *The third unsigned short integer in each Key Entry Set SHALL hold the number of values in the key (the Count). If TIFFTagLocation=0, Count=1 is implied.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet.keyID  *The first unsigned short integer in each Key Entry Set SHALL hold the KeyID.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet.shortKeyValues  *Following the KeyEntry definitions, the GeoKeyDirectoryTag MAY hold values for keys that are short integers. (NOT CLEAR, maybe the following: If TIFFTagLocation=0, then Value\_Offset contains the actual (SHORT) value of the Key, and Count=1 is implied. shortKeyValues specifies that value. )* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet.size  *Each Key Entry Set SHALL hold four unsigned short integers* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet.TIFFTagLocation  *The second unsigned short integer in each Key Entry Set SHALL hold the TIFFTagLocation. If TIFFTagLocation is 0, then the value is SHORT, and is contained in the "Value\_Offset" entry. Otherwise, the type of the value is implied by the TIFF-Type of the tag containing the value.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/KeyEntrySet.valueOffset  *The fourth unsigned short integer in each Key Entry Set SHALL hold the Value\_Offset. Value\_Offset indicates the index-offset \*into\* the TagArray indicated by TIFFTagLocation, if it is nonzero. If TIFFTagLocation is 0, then Value\_Offset contains the actual (SHORT) value of the Key, and Count=1 is implied. Note that the offset is not a byte-offset, but rather an index based on the natural data type of the specified tag array.* |

## Requirements Class MetadataTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/MetadataTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/MetadataTag.cardinality  *The private TIFF tag for holding XML metadata MAY be used more than once in a single GeoTIFF file.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/MetadataTag.ID  *The private TIFF tag for holding XML metadata SHALL have ID=50909* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/MetadataTag.Name  *The private TIFF tag for holding XML metadata SHALL be named GEO\_METADATA* |

## Requirements Class ModelPixelScaleTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag.count  *The ModelPixelScaleTag SHALL hold three values (ScaleX, ScaleY, ScaleZ)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag.count  *The ModelPixelScaleTag SHALL hold three values (ScaleX, ScaleY, ScaleZ)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag.ID  *The ModelPixelScaleTag SHALL have ID = 33550* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag.independent  *The ModelPixelScaleTag SHALL be independent of the Xposition, Yposition, and Orientation TIFF tags* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag.reversal  *Negative values of the ModelPixelScaleTag components SHALL indicate simple reversals of orientation between raster and model space (e.g. horizontal or vertical flips)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelPixelScaleTag.type  *The ModelPixelScaleTag SHALL have type = DOUBLE* |

## Requirements Class ModelTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/ModelTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTag.count  *If the ModelTiePointTag and ModelPixelScaleTags are defined the ModelTransformationTag SHALL not be used* |

## Requirements Class ModelTiePointTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag.count  *The ModelTiePointTag MAY hold any number of tiepoints* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag.count  *The ModelTiePointTag SHALL only hold one tiepoint that corresponds to the upper left corner of the image.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag.ID  *The ModelTiePointTag SHALL have ID = 33922* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag.independent  *The ModelTiePointTag SHALL be independent of the Xposition, Yposition, and Orientation TIFF tags* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag.size  *The ModelTiePointTag SHALL include six values for each tiepoint* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTiePointTag.type  *The ModelTiePointTag SHALL have type = DOUBLE* |

## Requirements Class ModelTransformationTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/ModelTransformationTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTransformationTag.count  *The ModelTransformationTag SHALL hold sixteen values* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTransformationTag.ID  *The ModelTransformationTag SHALL have ID = 34264* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTransformationTag.notAllowed  *The ModelTransformationTag SHALL not be used.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ModelTransformationTag.type  *The ModelTransformationTag SHALL have type = DOUBLE* |

## Requirements Class PCSCitationGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/PCSCitationGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/PCSCitationGeoKey.ID  *The PCSCitationGeoKey SHALL have ID = 3073* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/PCSCitationGeoKey.type  *The PCSCitationGeoKey SHALL have type = ASCII* |

## Requirements Class ProjectedCSTypeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey.EPSGProjection  *ProjectedCSTypeGeoKey values in the range 20000-32760 SHALL be EPSG Projection System Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey.ID  *The ProjectedCSTypeGeoKey SHALL have ID = 3072* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey.KeyValues  *326zz ““ UTM Northern Hemisphere, 327zz ““ UTM Southern Hemisphere (Where zz is the UTM zone number), Other PCS allowed by this standard (in conformance with DGIWG Geodetic Codes and Parameters Registry) 12 Present only for cartographic data. In this case, GTModelTypeGeoKey = 1 and GeographicTypeGeoKey is absent* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey.obsolete  *ProjectedCSTypeGeoKey values in the range 1-1000 SHALL be obsolete EPSG/POSC Datum Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey.private  *ProjectedCSTypeGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/ProjectedCSTypeGeoKey.type  *The ProjectedCSTypeGeoKey SHALL have type = SHORT* |

## Requirements Class TIFF

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/TIFF | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.bitsPerSample  *The BitsPerSample field in the TIFF Image File Directory defines the number of bits per component* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.byteOrder  *The first two bytes of the GeoTIFF file SHALL be equal to "I" (ASCII) (49 in hexadecimal) for TIFF files encoded using “˜Little-Endian”™ and SHALL be equal to "M" (ASCII) (4D in hexadecimal) for TIFF files encoded using “˜Big-Endian”™* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.DateTime  *The format for the field in ASCII type is “YYYY:MM:DD HH:MM:SS” with 24 hour time used for the hours and one space character between the date and time, and one terminating NUL character. The length of the string, including the terminating NUL, is 20 bytes. All dates and times shall be expressed in Coordinated Universal Time (UTC).* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.double  *GeoTIFF requires support for all documented TIFF 6.0 tag data-types, and in particular requires the IEEE double-precision floating point "DOUBLE" type tag.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.fileStructure  *A GeoTIFF file is a TIFF 6.0 file, and inherits the file structure as described in the corresponding portion of the TIFF spec.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.griddedValueDataTypes  *For gridded data (e.g. elevation data, matrices of lat/lon values, etc.), the range (data) values MAY be stored in additional representations to include 8-bit and 16-bit signed integer and 32-bit floating point.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.IFD  *There must be at least 1 IFD in a TIFF file and each IFD must have at least one entry.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.IFDCount  *The maximum nuber of IFDs in a GeoTIFF is two, with the second IFD only used to support a transparency mask.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.imageryValueDataTypes  *For imagery, the range (data) values SHALL be unsigned integer data, 8 or 16-bits-per-band.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.noPrivateInformation  *All GeoTIFF specific information is encoded in several additional reserved TIFF tags, and contains no private Image File Directories (IFD's), binary structures or other private information invisible to standard TIFF readers* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/TIFF.tagOrder  *GeoKey entries SHALL be written within the CoordSystemInfoTag in tag-ID sorted order.* |

## Requirements Class VerticalCitationGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCitationGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCitationGeoKey.ID  *The VerticalCitationGeoKey SHALL have ID = 4097* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCitationGeoKey.KeyValues  *WGS84 Ellipsoid, EGM84, EGM96, EGM2008, MSL height, MSL depth , or the name of the Sounding datum identified in DGIWG Geodetic registry (S-1 to S-40), or description os user-defined vertical CRS* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCitationGeoKey.type  *The VerticalCitationGeoKey SHALL have type = ASCII* |

## Requirements Class VerticalCSTypeGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.EPSGEllipsoid  *VerticalCSTypeGeoKey values in the range 5000-5099 SHALL be EPSG Ellipsoid Vertical CS Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.EPSGOrthometric  *VerticalCSTypeGeoKey values in the range 5100-5199 SHALL be EPSG Orthometric Vertical CS Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.ID  *The VerticalCSTypeGeoKey SHALL have ID = 4096* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.KeyValues  *4979 (WGS84 3D ellipsoid), 5773 (EGM96), 3855 (EGM08), 5798 (EGM84), 5714 (MSL height), 5715 (MSL depth), 32767 for other Sounding datums idenfied in DGIWG Geodetic registry, or user defined Vertical CRS* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.private  *VerticalCSTypeGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.reserved  *VerticalCSTypeGeoKey values in the range 1-4999 and 6000-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.reservedEPSG  *VerticalCSTypeGeoKey values in the range 5200-5999 SHALL be reserved EPSG* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalCSTypeGeoKey.type  *The VerticalCSTypeGeoKey SHALL have type = SHORT* |

## Requirements Class VerticalDatumGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/VerticalDatumGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalDatumGeoKey.ID  *The VerticalDatumGeoKey SHALL have ID = 4098* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalDatumGeoKey.private  *VerticalDatumGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalDatumGeoKey.reserved  *VerticalDatumGeoKey values in the range 16384-32766 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalDatumGeoKey.type  *The VerticalDatumGeoKey SHALL have type = SHORT* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalDatumGeoKey.VertDatum  *VerticalDatumGeoKey values in the range 1-16383 SHALL be Vertical Datum Codes* |

## Requirements Class VerticalUnitsGeoKey

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.angular  *VerticalUnitsGeoKey values in the range 9100-9199 SHALL be EPSG angular units* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.ID  *The VerticalUnitsGeoKey SHALL have ID = 4099* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.KeyValues  *9001 (meaning Linear\_Meter)* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.linear  *VerticalUnitsGeoKey values in the range 9000-9099 SHALL be EPSG linear units* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.obsolete  *VerticalUnitsGeoKey values in the range 1-2000 SHALL be obsolete GeoTIFF Codes* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.private  *VerticalUnitsGeoKey values in the range 32768-65535 SHALL be private* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.reserved  *VerticalUnitsGeoKey values in the range 2001-8999 SHALL be reserved* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VerticalUnitsGeoKey.type  *The VerticalUnitsGeoKey SHALL have type = SHORT* |

## Requirements Class VoidAreasTag

|  |  |
| --- | --- |
| **Requirements Class** | |
| http://www.opengis.net/spec/GeoTIFF/0.0/VoidAreasTag | |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VoidAreasTag.ID  *The private TIFF tag for defining void areas SHALL have ID = 42113.* |
| Requirement | http://www.opengis.net/spec/GeoTIFF/0.0/VoidAreasTag.Name  *The private TIFF tag for defining void areas SHALL be named GDAL\_NODATA. (GDAL\_NODATA is not defined in the GeoTIFF standard, however, this is an private TIFF tag that may be used for the purpose of declaring these values.)* |

# Media Types for any data encoding(s)

A section describing the MIME-types to be used is mandatory for any standard involving data encodings. If no suitable MIME type exists in http://www.iana.org/assignments/media-types/index.html then this section may be used to define a new MIME type for registration with IANA.

Annex A: Conformance Class Abstract Test Suite (Normative)

Conformance class: AAAA (repeat as necessary)

Annex B: Revision history

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date | Release | Author | Paragraph modified | Description |
| 2014-11-30 | 0.0 | Ted Habermann | Entire Document | Initial document |
|  |  |  |  |  |
|  |  |  |  |  |

Annex C: Bibliography

Association Adobe Developers. (1992). *Revision 6.0*.

Ritter, N., & Ruth, M. (1997). The GeoTiff data interchange standard for raster geographic images. *International Journal of Remote Sensing*, *18*(7), 1637–1647. doi:10.1080/014311697218340

Ritter, Niles, & Ruth, M. (1995). GeoTIFF Format Specification Authors : Acknowledgments : Disclaimers and Notes for This Version :

Wiggins, R. H., Davidson, H. C., Harnsberger, H. R., Lauman, J. R., & Goede, P. a. (2001). Image file formats: past, present, and future. *Radiographics : a review publication of the Radiological Society of North America, Inc*, *21*(3), 789–98. Retrieved from http://www.ncbi.nlm.nih.gov/pubmed/11353125

Annex D: The GeoTIFF File Structure (Informative)

The current GeoTIFF specification (GeoTIFF) includes a detailed description of the approach, the format and the semantics and values of the tags. The tag specifications are included as requirements in Clause 6. This Annex provides an overview of the structure of a GeoTIFF file.

GeoTIFF fully complies with the TIFF 6.0 specifications, and its extensions do not in any way go against the TIFF recommendations, nor do they limit the scope of raster data supported by TIFF.

GeoTIFF uses a small set of reserved TIFF tags to store a broad range of georeferencing information, catering to geographic as well as projected coordinate systems needs. Projections include UTM, US State Plane and National Grids, as well as the underlying projection types such as Transverse Mercator, Lambert Conformal Conic, etc. No information is stored in private structures, IFD's or other mechanisms which would hide information from naive TIFF reading software.

GeoTIFF uses a "MetaTag" (GeoKey) approach to encode dozens of information elements into just 6 tags, taking advantage of TIFF platform-independent data format representation to avoid cross-platform interchange difficulties. These keys are designed in a manner parallel to standard TIFF tags, and closely follow the TIFF discipline in their structure and layout. New keys may be defined as needs arise, within the current framework, and without requiring the allocation of new tags from Aldus/Adobe.

GeoTIFF uses numerical codes to describe projection types, coordinate systems, datums, ellipsoids, etc. The projection, datums and ellipsoid codes are derived from the EPSG list compiled by the Petrotechnical Open Software Corporation (POSC), and mechanisms for adding further international projections, datums and ellipsoids has been established. The GeoTIFF information content is designed to be compatible with the data decomposition approach used by the National Spatial Data Infrastructure (NSDI) of the U.S. Federal Geographic Data Committee (FGDC).

While GeoTIFF provides a robust framework for specifying a broad class of existing Projected coordinate systems, it is also fully extensible, permitting internal, private or proprietary information storage. However, since this standard arose from the need to avoid multiple proprietary encoding systems, use of private implementations is to be discouraged.

1. [www.opengeospatial.org/cite](http://www.opengeospatial.org/cite) [↑](#footnote-ref-1)